Introduction to custom anodized aluminum plate services
- Providing you with high-end, durable, and safe aluminum sheet surface solutions  - Product Overview
Anodized aluminum plate is a functional material formed on the surface of aluminum material through electrolytic process, which has excellent corrosion resistance, wear resistance, UV resistance, and decorative properties. Its surface can be customized with color, texture, and gloss, and it is widely used in the fields of architectural curtain wall, electronic devices, product decoration, automotive parts, bags, new energy projects, aluminum tiles for steel structure factories, and other areas.
Two, core contents of customized services
1. Material Selection
Different aluminum sheets are provided (such as 1060, 3003, 5005, 5052, 6061, etc.) to meet strength, ductility, and processing requirements.
Thickness range: 0.15mm~6.0mm, supporting customization of ultra-thin or thick specifications.
Width and height range: 1000mm~1800mm, supports cutting or custom specifications.
2. Color and Surface Effects
Color customization: Support for selection of colors from RAL, Pantone international color cards, or matching with customer's physical objects or design drafts.
Surface treatment: matte, glossy, brushed, sandblasted, patterned effects.
3. Dimension and Shape Machining
Accurate cutting: flying shears, strip feeding, laser cutting, CNC shearing and other shape requirements.
Bending and stamping: can be equipped with deep processing services to meet the assembly needs of structural components.
4. Anodizing Process Parameters
The thickness of the oxide film: 5μm~25μm (adjusted according to weather resistance requirements).
Hole sealing: Enhance anti-pollution performance and extend service life.
Three, Customization Process
1. Communication of requirements.
The client provides the application scenarios, design drawings, or samples, and clearly defines the performance and appearance requirements.
The technical team assesses feasibility and recommends materials and processing methods.
2. Sampling Confirmation
Within 3-7 working days, samples will be provided, supporting multiple adjustments until satisfaction.
3. Batch production
Using automated production lines, strict control of the uniformity of oxide film and color difference.
4. Quality inspection and delivery
Through salt spray testing (ASTM B117), hardness testing (HV), colorimeter detection, etc.
The packaging is scratch-resistant and shockproof, supporting global logistics distribution.
Four, Service Advantages
1. Technical Strength
With over 20 years of industry experience, equipped with advanced oxidation production lines and testing equipment.
The engineering team provides one-on-one technical support.
2. Rapid Response
Small batch orders will be delivered in 7-15 days, and urgent requirements can be expedited.
3. Flexible customization
Support personalized logo engraving, customized colors, special protective coatings and other value-added services.
4. Environmental Protection Compliance
Compliant with RoHS and REACH standards.
Five, Application Areas.
Architectural decoration: curtain wall, ceiling, elevator hall, exhibition hall...
Industrial design: signage, instrument panels, equipment enclosures, luggage shells, radiators...
Consumer electronics: phone and computer cases, smart home panels...
In the field of transportation: road signs, high-speed train interiors, ship interior decorations, new energy vehicle components, etc.
Six. Cooperation Guarantee
Sign a confidentiality agreement to protect the client's design intellectual property rights.
Provide lifelong technical consultation.
Contact Us
If you would like to learn more details or get free samples, please contact customer service:
📞 Telephone: +008613825560000
📧 Email: service@xxx.com
🌐 Official website: www.xxx.com
Innovative choice with peace of mind! Achieve your creativity with professional craftsmanship!
Customized anodized aluminum plates, blending quality and aesthetics perfectly.
Customization process:
Inquiry → Requirement Submission → Sampling → Confirmation → Scheme Quotation → Contract Signing → Production → Quality Inspection → Delivery → After-sales
Customized advantages of anodized aluminum plate core
- With professional, flexible, and reliable services, empower your innovative design.
One, leading technology, quality assurance.
1. Precision engineering control
Using a self-developed anodizing electrolytic coloring production line, precise control of the concentration, temperature, and voltage of the electrolyte is achieved to ensure uniform thickness of the oxide film (tolerance ±1-2μm), with consistent aluminum natural color within ΔE≤1.0; color consistency within ΔE≤2.0.
2. Full-process detection system, equipped with laboratories and testing centers!
Equipped with various measuring instruments, colorimeters, film thickness gauges, UV aging test chambers, constant temperature and humidity chambers, electrochemical performance testing equipment, etc., the entire process executes over 10 quality inspections.
3. Strong adaptability of materials
Covering aluminum alloys from series 1 to 7 (such as 1060, 5052, 6061), meeting different requirements of strength, electrical conductivity, and weldability.
The thickness customization range is wide (0.3mm~8.0mm), supporting ultra-thin sheet high-precision bending and thickened plate heavy load-bearing scenarios.
Two, flexible customization, efficient response.
"Small batch + quick delivery" mode
Zero threshold ordering: Starting from 500KG, reducing the cost of trial and error, suitable for new product development and niche designs.
Rapid prototyping: sample out within 1 day (conventional process), supporting "sample + mass production" one-stop service, reducing project cycle by 30%.
2. Personalized design with full coverage
Color freedom: matching 2000+ standard color codes such as RAL, Pantone, supporting metallic texture, matte, gloss, brushed, sandblasting mixing effects.
Texture Innovation: Customizable wood grain, stone grain, wire drawing, sand blasting, embossing, 3D relief and other special surfaces to enhance product added value.
Integrated functionality: combined with conductive layers, self-cleaning nanolayers, and other functional treatments.
3. Deep processing support
Offering a full chain service from board to finished product: slitting, flatting, laser cutting, CNC engraving, bending welding, assembly packaging, reducing the collaborative costs of multiple suppliers for customers.
Three, service advantages, worry-free throughout the whole process.
One-on-one technical advisor
Senior engineers will follow up throughout, providing free technical consultation from product drawing optimization, process material selection to installation guidance.
Support on-site factory inspection, video inspection, and transparent production process.
2. Global Delivery Network
Domestic 24-hour logistics direct delivery, overseas cooperation with DHL, FedEx and other special lines, providing DDP door-to-door service (including customs clearance, tax payment).
Urgent orders can be expedited for delivery within 10 days (advance filing required).
3. After-sales guarantee system quality traceability mechanism: Establish unique product identification (such as batch number, production date, process parameters), achieve full traceability from raw materials to finished products; archive key test data (such as film thickness, salt spray test results), facilitate rapid location of after-sales issues.
Warranty and Commitment: Clearly define the warranty scope (such as oxide film, corrosion, fading) and non-warranty situations (such as human damage, improper installation) according to the application scenarios (such as building curtain walls, industrial equipment, appearance products).
Spare parts and inventory management
Reserve common specifications of aluminum coils, establish a supplier collaborative inventory mechanism to cope with urgent demands.
Data cloud archive: Customer order parameters are encrypted for storage, supporting quick reorder within 3 years without the need for repeated communication.
Four, cost optimization, value enhancement
Inventory and loss control
Produce on demand, zero intermediate inventory, reduce customer capital occupation.
Waste material recycling service: Free processing of waste materials, environmentally friendly and compliant, and reduces customer management costs.
2. High cost-effectiveness.
Procuring aluminum-based materials in large scale, the cost is 8% to 15% lower than the market price.
The process integration (such as oxidation + cutting + bending) saves more than 20% of the outsourcing processing fees.
Five, environmental protection compliance, sustainable cooperation.
Green Production Certification
Complies with RoHS, REACH, ISO 99001 standards.
Provide QUALANOD certification and SGS environmental testing report to help customers pass export certification.
2. Low carbon solutions
Promote renewable aluminum materials (recycling rate ≥90%), support carbon footprint tracking, and meet ESG strategic requirements.
Reasons for choosing us.
✅ Strong technical capabilities: Leading the industry in process precision, with quality that can withstand extreme environmental tests. 
✅ Super flexibility in service: Efficiently delivering orders from 1 square meter to tens of thousands of tons, offering standard colors to creative designs. 
✅ Sustainable cooperation: Simultaneously reducing costs, increasing efficiency, and fulfilling environmental responsibilities, adding value to your brand.
Start your exclusive journey of metal aesthetics with immediate customization!
📞 Contact Hotline: +008613825560000
📩 Business cooperation: sales@xxx.com
Let every piece of aluminum plate be the quality statement of your brand.
